Version 0.9.25 (21.05.2000)
=================================
* I've changed version numbering of the SemTel to have same system of
  numbering on all of my programs.
* 16bit revison is no longer supported, last is 0.920.
* Printing:
    - I've rewritten direct printing functions, I stoped using function
      Escape(), which is not implemented in many of printer drivers.
      Now I'n writing directly to devices LPTn a COMn.
    - I cause that you have been using direct printing, you have to check
      configuration. Now is printer in direct mode identified by port name
      not by MS-Windows name.
    - I added new cmdline switches:
        -SavePrintedPRNData <FileName> allow save data exactlly in format
         in which they were sent to printer.
        -SaveReceivedPRNData <FileName> allow save data exactlly in format
         in which they were received by SemTel, it mean before any
         conversions.
* SSL:
    - Is posible to use encrypted connection from begin of the connection.
      No telnet negotiation is needed for establishing encrypted connection.
      Due this feature is not required to install specialized telnet daemon,
      stunnel is enought.
* On program terminaing an error happen if wasn't posible to write into
  INI file - fixed.
* Was posible to enter non existing terminal name - fixed.
* Messages in window "Select connection" were wrongly terminated - fixed.
* Emulation fixes.

Version 0.920 (18.12.1999)
=================================
* Printing:
    - Characters TAB and NL were not printed on printer - they were always
      printed on the console.
    - It is posible to disable displaing dialog window "Profily tiskáren"
      before printing.
* Telnet emulation:
    - Fixed bugs in emulation telnet options TERM and NAWS.
* New command line switch -UserName, -U allow you specify user name
  which will be sent to host after detection of string "ogin:".
* In menu "Connection" there is new item "Duplicate", after selecting
  SemTel will open new connection to same system as in parent window.
* From now I will use GnuPG. It is OpenSource alternative to commercial
  PGP. You can get more information from http://www.gnupg.org.

  My personal public key is:
      pub  1024D/03AC066B 1999-12-09 Jan Tomasek (CZ-7508180295)
           Key fingerprint = 8F9F 59CE 1F3E 7121 2042
                             AA11 BA4D 9E32 03AC 066B
      sub  2048g/7F63B99E 1999-12-09

      -----BEGIN PGP PUBLIC KEY BLOCK-----
      Version: GnuPG v1.0.0 (GNU/Linux)
      Comment: For info see http://www.gnupg.org

      mQGiBDhQBUcRBACeZHmpXuRFLi4EOL3c9OwBSivT+cxQhZq5BS3Lub3WQRy8Kf93
      MLW1jxS9baEzfT4feZ2ZBYAELOgylLzhxsE0Tc2kvdru/kxFhBlHdBfj/jCaiIBr
      v6WzlTuNcm0AZv6b511bx0xkutQCgtEZoMzO5mkF9cKPmqXFhn0MQH2tKwCgvO5M
      H3/65KaR+peZ/1tnmy5CRv8EAIMZnmnLY1eVP4EnNiTIhOudxhfRrmt2W/9gYUHK
      k9vnTEsDlbFX4RTDcA9mI/grCs9vMrPT/obXkUn09Yiouz0JOeXodPLGLh5c7Nhz
      xaRE827leEA2H9fjNocjLRm161d/HTRuVcGuQRhMJAM0YVcWD9m646uV6+Dwv17c
      qu9LA/9U6AQd0EHjgxD2o01viHzaLznpFZrnvlwuZhEhfcz0vvRmNFV/hdevNbjn
      XjCTCGtIu0BWDBEfexqOrMZE5UK91KvfFxeAUiTJajzl4IHxvsPOukjYLuD+f0p6
      uSEzL3u7UJQJRezKhx0z0i/ZB4SwOIkN29ZfdCkvc3qVc4//sbQbSmFuIFRvbWFz
      ZWsgKENaLTc1MDgxODAyOTUpiFUEExECABUFAjhQBUkDCwoDAxUDAgMWAgECF4AA
      CgkQuk2eMgOsBmvt+wCglLIgOu8Qknp47f0B01kXouIftnsAnRvxc6u9jxxUTap4
      scDmV3fLgmSauQINBDhQCckQCADPduP2M3aV9dVZxvBOxwB+N/K/S9AERtnD8XcA
      gBYHPRiwO9Umf0twyxEO7LRDQyxUsPSZE0lqJR8scSS8m7JEAj2CS17KoR6y2Wdg
      R3glxjk/CDEcQ4++p/HGGc2qY/MvHiYZjZmJ3TazrOC5ri1mQvSCKOJLASqPsWqK
      2Yq2nXo6fUgoAj1KWdjMcL4q19IqwRdOElGylHDIDMcCD0/WC7+QF2b+8GoHvOU+
      B53Vg5oNuEsvxhAx3Vyj8+mskOcnxNW6IT+y0FnfFXPY3L3iNGTdBtbrnzTu5VSw
      oD0bwwRgIPw45WpEUOKh0WtGBcVgEmgFffF3Il9ZaKNvM3qDAAMGB/46xGWGEv3f
      xQaRPflLfL4AX6OkjR/qY9+Zo1gILlCnuc78dM2KVlq5fDuj/8GtCdGVfpiZfqe1
      VGujAeFsPG0McnOU2VybiObjMsRw+nv5s3tWyGL2NtFG2Pv2vGEaCpQUvbZxKHdQ
      kBoqCiDZl1kxds0G4nsR8TCZoyA7BMZrf9fZb4coOu1ma1sqa/6uUqseiKmAbSoo
      UsJYBtnwv2ANwy5xytZj5cgTrftCgvJzb7RWpg14zo6X711Xb8MNBU7/nJKRcZ6J
      3sphXI2ZfBApwicM6+r3VMQoWRvBs3bh2/poT20uA/kG35Ku3jhL1y2MtH0XujBE
      d6opFJzXBxOEiEYEGBECAAYFAjhQCckACgkQuk2eMgOsBmuf+ACfWIt31D0W7P2Q
      1Nhaq2P5p9teH+EAn0DOTj9QiI/hYKIhEyQjuvAT+EJ3
      =GS+D
      -----END PGP PUBLIC KEY BLOCK-----

  Public key for SemTel:
      pub  1024D/B028472C 1999-12-10 Jan Tomasek (SemTel)
           Key fingerprint = 3006 AC57 6E6D 6EED FB06
                             4455 1560 3BB4 B028 472C
      sub  2048g/DA20CF35 1999-12-10

      -----BEGIN PGP PUBLIC KEY BLOCK-----
      Version: GnuPG v1.0.0 (GNU/Linux)
      Comment: For info see http://www.gnupg.org

      mQGiBDhRLmURBACmiEZ2QHjV9BQCbaueJZuWFN7oJxC5PikujrxoMBy85o0CU9Wv
      bfFpYbv2Qn2ZdJEJ47rN72lwEKTro1iut/HJcy/EybgEUs3moBqb9axFnIFTeGVm
      6oaGn1wgQWg7aHw5NgpCF9r25OpIMr9PhQl2+grsGLyC9kZIbFhgeIFTRwCgw2Gp
      fseZXZ1f5HU21jajfNDfpmsD/26Sn4AismRfYaEBEEHGLbC7SM5a7WYeUt7w+Yv7
      YbgOD3k0aEDeD5sLxAmPaMHfaD1KfBWggQunIuJCU67xdDsaWFdogUbEV0fYKw0y
      hptg/Z20xgFv5fWbf32R2QGTtyoZwmMwMOyByVgaguXYPEiLPVzabI5exmhXzVdJ
      i3AcA/0ZlU7R9TMFpafawEzNiMSSMj5vkHBziiJFWAGcvAmV1Tn9yfeUx5SpNZQm
      yAgBi/CDXP4+ki9i6o8DrVNJky4ZuVCfakMiHMBfH17WRd2xg24BHFADfCVvRQ2Q
      mrEQZ9wOL6NDlHC5UI3E3tjs1/2bRyaxmaf1wUeHpJRTh5cDl7QUSmFuIFRvbWFz
      ZWsgKFNlbVRlbCmIVQQTEQIAFQUCOFEuZQMLCgMDFQMCAxYCAQIXgAAKCRAVYDu0
      sChHLH4qAKCegTBuQw3keS6xVOVuGvmPyJ0YOwCeP/EGa1ZQCoSw89ptCgreg7Ft
      bI6IRgQQEQIABgUCOFExiwAKCRC6TZ4yA6wGa6PpAKCGTQ+dHzrEqFGOVsNFfeml
      I5xD8gCfeYSx+wM5KZGQ/4OnDt/OO0BAnhq5Ag0EOFExVhAIANm5y1e1PwUDeMe8
      ZLidbu9zg0vtw1ADlAazkJ5RFzhFIQJRGAurkkOM54rnvTj09yP7qXhUrf8pPFn8
      ytTkT9beDqAh9/V/bc07/QhubOrVYE7QSXQsbp/fM1IIfs6IXzJ1+/5sdevDuy70
      l+BhDh8FDS0lZLCA7l3WrQ2zbDW6oGVKb8glCdD1MaUGXK0EAmMnvPx8/ARpZOsA
      Mus0cFUuEnHH7lUZ52YkH19Ev1PCAt4fwGr0yyjEP160Ar+LN5b2XUyzIZlFPawj
      T0oXUVSjpKwv6lM6S5Il6dKkw5eCH5zqEYjDjzKg/MtyyzfKD6Mtx8MMjNqalQfi
      gnBRX3sAAwYH/3oB0Mri7uTbC0mgiQb4j4A+5EJUOPD5W5Vspz40/KI/LwIYbwBC
      dwslhK8jxXYiYhQmiDZp0ul6vGMNSvSKTJNbCMZcb9vXo3IaR4wI4kRlzAHlkKxN
      7sZEaSZm4DVEw9W5LrpBG4EuoNeLx+oxl39SrRJWVSnlnpSJNZ64eqhbsxD5JfuG
      rjaCUgx3Nfey8QW5PNx0dFDRQ+/q93EiptXuV+cyd+sDwEpobj0YKjMJJhJml5Sz
      X6LEVDIW3qG0T7W/4izO/DyrdFNkiu9OWQ1s+M5eh9LcblKckQdFfhn5GfUsvIBS
      Ld+bQANeMhsay5dDLDL7/XoSB2Io5ZQQ3q+IRgQYEQIABgUCOFExVgAKCRAVYDu0
      sChHLD+6AKCqDUlI+D8xNDqsV/tM8xUH8u3R/QCeKOeE1dCV+misQfaDt1Jg8ujU
      qPs=
      =By2B
      -----END PGP PUBLIC KEY BLOCK-----

Version 0.919 (21.11.1999)
=================================
* OTP calculator:
    - will warn you before password expire, warning treshold can be set
      from INI file - section [Global], item 'OTP.Minimum=1;20'.
      Default value is 20.
* Printing:
    - Fixed problem with czech printing mode on some Windows 95 and NT.
    - Button Cancel will from now work as you expect.

Version 0.917 (05.06.1999)
=================================
* OTP calculator didn't convert 'seed' to lover case - fixed.
* FTP server didn't work in vesion 0.916 - fixed.
* Environment:
    - Fixed bug in sending parameters of environment.
    - Default parametr SYSTEMTYPE=Win32 can be now deleted.
* Is posible to select color for highlight selected area. You can choise
  betwen fillin area or only drawing edges. 
* Selected color of cursor is now correct at all backrounds - only in 32bit.
* Program 'enc2' was recompiled by MS VC 6.0, now it works faster and
  didn't require cygwin19.dll.

Version 0.916 (12.04.1999)
=================================
* An empty page was printed after print in windows print mode - fixed.
* In direct print mode form feed characters were ignored - fixed.
* Empty lines were not printed - fixed.

Version 0.915 (15.02.1999)
=================================
* Fixed bug which cause SemTel's crash under WinNT 4.x. Problem was
  caused by section with empty name ''.
* I add to official definition of 'ansi' terminal definition of keys
  Shift+F1 .. Shift+F12 and Ctrl+F1 .. Ctrl+F12. (File ansi_enh.trm)
* During startup SemTel logs detailed info.
* Fixed bug in releasing code pages.

Version 0.913 (09.02.1999)
=================================
* In definition of terminal 'ansi' was written "ignore = \x40", that cause
  that SemTel didn't display character @. Please, execuse my bug.
  VT100:
     - terminal definition was split into few files
         1. vt100.trm     - main file
         2. vt100_dl.trm  - terminal definition coresponding to definition
                            of vt100 on Debian/Linuxu
         3. vt100_enh.trm - sequentions which are not in definition on
                            Debian/Linuxu
     - ArcTel a telnet from Windows are transmiting after Up-Arrow key
       sequention "\E[A". SemTel is transmiting "\E0A", which is, I hope,
       correct. But some system (IS of our faculty - Oracle) requires
       first one and others requres second one. I thinking about solution.
* Is posible to change sequention for key ESCAPE. I forgot it in last
  release.
* Version 0.912 doesn't send key kombinaci CTRL+A. Fixed.

Version 0.912 (31.01.1999)
=================================
* SemTel now supports VT100 terminal - this ability is in intesive
  testing please reports any problems.
* While closing windows(s) with active connection you will be always
  asked by SemTel for acknowledge. SemTel suports this three ways for
  closing window:
    - ALT+F4 ... standard Windows feel. After positive ansver to question
      "Do you wish to close active connection?" is closed window where
      combination was pressed. This question will be shown only if
      in window is active connection.
    - CTRL+F4 ... after same question is closed active connection and
      is showen information about this fact. Window is destroyed
      only if SemTel have other window with active connection.
      This key can be changed.
    - ALT+X ... after question with list of all active questions, will
      SemTel close all conections and terminate itself. This key can be
      changed.
  Notice: If you are using SemTel for some days you have changed
  CTRL+F4 to ALT+F4 this is cause why is not posible to close
  window where isn't active connection by ALT+F4. For correcting
  this you need change assigned key. For menu command "Connection/Close"
* In "direct printing mode" was some time printed one empty sheed.
  One FF (Form Feed) is sent by remote system second add SemTel - fixed.
* Many users ask me for simples way how to establish new connection.
  I add function 'Quick connect', this function allows you do that
  task you will asked for host name, port number and name of connection
  which will be used for seting up SemTel.
* Now is posible to use bold face of fonts. Font "Courier New" realy looks
  better in bold face. WARNING: If selected font have not bold face
  system will select some similar font - result is typical terible.
* I divide lng file into two files. With this change should be simplest
  localisation of SemTel. SemTelCZ.lng - Czech strings, SemTelEN.lng -
  English strings. SemTel.lng contains link to all known languages.
* New commands for terminal definition:
    - 'll' .... move cursor to first column last line
    - 'rep' ... n-times repeat last character
    - 'ind' ... "scroll forward" increment by on y cordinate of cursor
                if cursor goes over end of scren SemTel will scroll. 
    - 'csr' ... "scroll region" will change active screen size. Rows before
                and after will be untouched.
* Is posible to redefine whole keyboard:
     - Numeric keypad, in terminal definition is posible to use this
       keys with all combinations with CTRL, SHIFT, ALT:
           k_N_NumLock, k_N_Divide, k_N_Multiply, k_N_Minus, k_N_Plus,
       following keys are correctly recognized only if NumLock is on
           k_N_Decimal, k_N_0, k_N_1, k_N_2, k_N_3, k_N_4, k_N_5
           k_N_6, k_N_7, k_N_8, k_N_9
     - For refinition of letter and mubers use this variables:
           k_A, k_B, k_C, k_D, k_E, k_F, k_G, k_H, k_I, k_J, k_K,
           k_L, k_M, k_N, k_O, k_P, k_Q, k_R, k_S, k_T, k_U, k_V
           k_W, k_X, k_Y, k_Z, k_0, k_1, k_2, k_3, k_4, k_5, k_6
           k_7, k_8, k_9
       and left keys (name, character, Windows scan code):
           k_LQuote ..... ` 192
           k_Minus ...... - 189
           k_EQU ........ = 187
           k_Backslash .. \ 220
           k_LBracket ... [ 219
           k_RBracket ... ] 221
           k_Semicolon .. ; 186
           k_RQuoute .... ' 222
           k_Comma ...... , 188
           k_Decimal .... . 190
           k_Divide ..... / 191
           k_ScrollLock
           k_CapsLock
     - If you want to work with this, you need known:
           1. In this mode isn't difference betten small and capital letters
              (a, A is only A)
           2. Scan codes if keys k_LQuote .. k_CapsLock if found experimentaly
              I didn't found them in WinAPI help.
           3. I didn't implement this for creating localized keyboard. I
              provide this capability for simplest adaption SemTel to
              application on host system.
     - In file ./trm/keyb_enh.trm are listed all suported keys.
* Fixed bug in 'ambc' processing 
* Fixed some small bugs

Version 0.911 (04.01.1999)
=================================
* Version 0.910 sometimes becomes frozen - fixed.
* In window title is showed state of socket (connecting, connected,
  ... closed)
* In terminal definition is now posible use sequences as in printf()
  in C language C. Supported sequences are:
    - '\\'        backslash
    - '\b'        backspace
    - '\E', '\e'  escape
    - '\n'        new line - CRLF
    - '\r'        carriage return - CR
    - '\t'        tab
    - '\nnn'      insert character with value nnn decimal
    - '\0nnn'     insert character with value nnn octal
    - '\0xnnn'    insert character with value nnn hexa
    - '\xnnn'     insert character with value nnn hexa
    - '^X'        insert character byte('X')-byte('A')+1; X is from
                  interval 'A'..'Z'

Version 0.910 (12.12.1998)
=================================
* FTP server does not use port ftp-data for data connections, it was
  reason why was not posible to put/get data from computer after
  firewall. Fixed.
* If remote system start fast transmision of big amout of data
  SemTel cause total lost of operating system resources and in
  result it cause that OS becomes frozen until remote host stop
  transmision. I get off this problem, now is SemTel working
  corectly. You can without problems continue in work in diferent
  window, close SemTel ...
* In menu help is new item "SemTel's www pages"

Version 0.909 (06.12.1998)
=================================
* If you try to paste from emply clipboard SemTel will cause Access viloation
  exception - fixed.
* From window 'Connection parameters' I remove gradient title - I consier that
  it decrease program stability.
* I changed default exception handler. Window with information about exception
  was changed. And above all is here no posibility to write messages about
  exceptions to disk file. You can use this cmd line switchs for controling
  this ability:
        - '-Debug <File name>' switch on writing messages to disk
        - '-DebugLevel <0|1|2>' amount of written informations:
             0 ... nothing will be written
             1 ... standard level - only exceptions will be written
             2 ... detail informations - level 1 and will be written info
                   about enter/leave of selected functions

Version 0.908 (01.11.1998)
=================================
* Forms for creating order bill and showing PGP key.
* I fix bug which cause GPF exception if was pressed button
  'New connection'. And next GPF was raised at end of SemTel with
  conditon that you add new connection definition.
* In terminal definition I change 'k_ent=^M' to 'k_ent=^J^M', it means
  that after pressing enter key will SemTel transmit CRLF not only CR.
  With this change is posible to use SemTel for debuging of services
  as is SMTP, POP3, HTTP ...
* I fix some minor bugs

Version 0.903 (xx.08.1998)
=================================
* Added support MD4 algoritmh in OTP (S/KEY) calculator.
* changed faq:
        otp.txt

Version 0.902 (26.08.1998)
=================================
* Fixed bug created in version 0.901, this bug cause that SemTel
  on some system printig unrecived characters.
* new faq:
        otp.txt - "OTP - One Time Password?"

Version 0.901 (19.08.1998)
=================================
* This version is vailable only for Win32, I must fix some nějaké
  probeml in Win16, after that I will release version for Win16.

* Support for crypted connection trought SSL - read faq/us/ssl.txt
        - is posible to set SemTel to do
                - will use/not use crypted conection in depend on
                server ability
                - will always requre cryped connection if server
                refuse SemTel will close connection.
        - in document faq/us/ssl.txt is writen where is posible to
        get telnet damon.
        - I add Purple LED diode for signalizing if connection is
        cryped.
	- FTP doesn't allow crypted connection, at this time.

* Fixed problem in parsing ESC sequention. 
* Sequention with character ¤ have lowest priority. If is in parsing
  tree found, for example, \E[¤A and \E[1A action for \E[1A will be
  executed more info in faq/us/termtype.txt.
* New terminal abities:
        - 'mc' replaced by 'mc4' a 'mc5', switch on/off printer
        - 'ceos' replaced by 'ed', to be more similar to teminfo
        - direct access to color switching for "Open Ingres from
        Computer associates", see faq/us/termtype.txt, ansi.trm.
        - 'am' automatic margins
                - 'ambc' when check automatic margins, see ansi.trm,
                this has a relation to 'top' problem described in last
                version.
        - 'ht' tabulator to next hw position (8 character).
        - 'el1=\E[1K' delete to begin of line
        - 'cr' move cursor to begin of line ^M=13 dec
        - 'bel' beep
        - is posible redefine sequentions for keys with CTRL, SHIFT
        and ALT. Look at ansi.trm. Some combinations are not allowed
        by OS for example (CTRL+ALT+DEL)! Length of sequention is
        limited to 50 characters in binary form.
        - by default is assigned (at this time only)
                - ALT+F12 = logout^M
        - 'k_cbt' deleded - same as SHIFT+TAB
        - 'smacs', 'rmacs' - switch on/off semigraphics
* Implemeted telnet option EVIRONMENT - NEW and OLD version. 
  Allows trsnsport to host constant, local OS param or SemTel param.
  For SemTel param at this time only - SEMTEL_LOCAL_IP.
  More info is in faq/us/environ.txt
* Is posible to change cursor color.
* Is posible to send file before/after printnig for activating and
  deactivating priter.
* SemTel allows print debug informations about establising connection
  (telnet options negotiation).
* New faq.


Version 0.882 (xx.07.1998)
=================================
* If computer has more than one IP address, dialog for select one
  will be displayed after command 'Insert local IP address'.
* I fixed caret.
* Fixed problem with command 'top'. Not exactly see version 0.901.
* New command lines arguments:
        - CS ................ SemTel will start with dialog
                              'Connection select'
        - C ConnectionName .. SemTel will automaticaly connect to
                              entered predefined connection. If
                              ConnectionName isn't valid dialog 
                              'Connection select' will be displayed.
* While resizing window by mouse is showed valid future size. Like
  console windows in Win95/NT. Only for Win 95+/NT4.x+.
* New faq.

Version 0.87 (12.06.1998)
=================================
* FTP server wasn't able to process user rights for more than
  one directory. Fixed.

Version 0.86 (02.06.1998)
================================= 
* Is posible to control ScrollBar by keyboard, see v0.60.
* Is posible to copy from any console's page.
* Fixed cursor's position display.
* Local echo (password should be visible!), different color.
* Line mode: entered characters are showed on status line and should
  be send by key <ENTER>, function keys are sent immediately. 

Version 0.85 (18.05.1998)
=================================
* I fixed probelms with FTP server under Win311
* 32bit version doesn't work without printer. Fixed.

Version 0.84 (12.05.1998)
=================================
*  Fixed some small bugs.

Version 0.83 (11.05.1998)
=================================
* While exiting SemTel in SuperUser mode was produced a GPF. Fixed.
* Because DOS has short command line I make some command shortes:
	-SuperUser    = -S
	-MainINI      = -M
	-LocalINI     = -L
	-LoadDialogs  = -D
* In version 0.81 was problem with encoding clipboard content while
  paste (caused by changes for 32bit compiler). Fixed.

Version 0.82 (11.05.1998)
=================================
* I fixed some problems with fonts under MS-Windows 3.1x.
* FTP server stil doesn't work reliabily under MS-Windows 3.1x.
* SemTel is available in 16 and 32 bit version.

Version 0.81 (30.04.1998)
=================================
* Window "SemTel" which you can see if you switch betwen tasks by 
  ALT+TAB is now hident.
* GPF problem in FTP server was fixed, but new one is here. Data
  connections aren't closed under Win311 and Trumpet winsock 2.0B,
  this causes that FTP server is in this system configuration
  unusable. Please test it with your system and refer me.

Version 0.80 (27.04.1998)
=================================
* While reading ans file SemTel crash with GPF message. Fixed.
* Now is posible to switch betwen SemTel windows by ALT+TAB, but! is
  visible window "SemTel" whitch I'm using as main application window.
  I'm trying to hide it.
* Now is available FTP server and printing capabilites. Both are
  configurable from "Connection parameters" window.
* F T P S E R V E R
	* I've written FTP server witch you can run on your computer
        and transfer by it files to host system. Of course is posible
        to run FTP server on host side, too. But it's less safetely
        for host system.
	* Server is connectable only for one user. Instruction to use:
		* Start FTP server
		* Start FTP client on host side and enter him your IP
		address, you can use command "Insert local IP
                address".
		* Doesn't matter on user name, simply type something.
		* Insert password by command "Insert FTP password".
		* Now you can work. Remember rules are changed, your
		computer is server and host is client!
	* PASSWORD, consist of eight characters a-z, A-Z, 0-9. It's
        created by random number generator. Random generator is
        initialized by count of messages received by main window. At
        time when you enter command "Insert FTP password" is password
        generated and set to FTP server and sent to host. After user
        login is password changed.
	* FILE SYSTEM, virtual file system isn't supported at this
        time.
		* Home directory, startup directory.
		* Read only directories, FTP client can read all in
                listed directories. Directories are separated by |.
                If you uncheck checkbox, all data in your computer is
                readable for FTP client.
		* Read-write directories, FTP client can override all
                in listed directories. Directories are separated by |.
                If you uncheck check box all in your computer can be
                deleted.
		* In lists you can type max 32 directories and in all
                it must be shortest than 255 chars. 
	* Working corectly with main and local INI.
* P R I N T I N G
	* SemTel can redirect it's output to printer if server
        require it. Sequence for printer is started by \E[5i and
        closed by \E[4i.
	* At page "Printer profiles" you can predefine some profile
        from witch you can quickly select one before print. Last
        selected profile is default profile.
	* Charset hacking is same as console charset hacking. You can
	select host and client (printer) charset and substitution
        table for line art. You can select if you wish to replace LF
        by CRLF
	* Access mode:
		* direct - fonts of printer are used, in Windows
                printer quele isn't visible valid document length.
		* windows - fonts of Windows are user, in W.p.q is
                visible valid document length.
	* Working corectly with main and local INI.  

Version 0.70 (20.04.1998)
=================================
* Paste from cliboard is posible by midle or right mouse button.
* C O N F I G U R A T I O N
	* SemTel is now able to work with two INI file, this should be
	usefull on LAN. One file is main(prepared by superuser) and
        second is local where is saved user's configuration.
	* I rewrite window "configuration", now it looks as
        equvivalent window in Netscape Comunicator. In near future
        I'll add printers configuration and reverse FTP.
	* Main INI file: created by superuser by SemTel in special
        mode. This spec. mode is activated from command line by
        parameter "-SuperUser". In this mode you can prepare
        predefined connection for your's users, you can specify
        whitch parametr can user redefine, this is done by checkbox in
        right top corner of options group. By default is this file
        called SemTel.ini and is at same place as EXE. You can specify
        another place by command line switch 
	"-MainINI <FileName>". Window's positions in this file are
        ignored.
	* Local INI file: created automatically by SemTel at end. In
        this file is stored windows position an sizes, subst.tables
        for line art, user defined connections and parts of predefined
        connections whitch can user modify. By default is this file
        called SemTel.ini and is in Window's folder. You can specify
        another place by command line switch "-LocalINI <FileName>".
	* Your old INI you can translate by program 
        ./tools/ini2ini.exe, argument is name of your INI. This
        program will translate this sections:
		* Connections => NewConnections
		* LineDrawSubstitutionTables => LineDrawSubst
	After this you should delete old sections Connections and 
	LineDrawSubstitutionTables.
* L A N G U A G E S, SemTel speaks czech or english and can encode
betwen arbitrary encoding model (ISOxxxx-CPxxx ...).
	* SemTel.lng: file with messages in czech and english. By
        default at same place as EXE. You can specify another place
        by command line switch "-MSG <FileName>".
	* SemTel.bnc: file with encoding tables, for n enoding models
        it contains n^2-n tables. Any user can create this file by
        program enc2bin from ./tools/enc.zip. That program takes as
        input *.ENC files where are in text mode writen positions of
        national characters. By default at same place as EXE. You can
        specify another place by command line switch "-CP <FileName>".
        If this file doesn't exist SemTel can continue in work.
* F O N T S
	* I had used font Terminal from standard MS-Windows
        distribution.  But with this font is problem, if you start
        SemTel, then MS-DOS window and after while you close MS-DOS
        window SemTel will lost font Terminal and will continue with
        font System but with Terminal's metrics.
	* That's main reason why I searched for new font for SemTel.
        I found fixed fonts form BIZNET for Linux. I put this fonts to
        ./tools/fonts.zip. There you will found direcory named CP1250
        where are translated fonts to CP1250 (original distribution
        is in ISO-8859-2). If you don't need CP1250 an you need line
        art you must use CP1250 fonts because in original are line
        draw characters are in control characters area.
* All dialogs will be allocated on demand, you can specify that you
  wish to load them at start by command line argument "-LoadDialogs".
* SemTel now allows to run several copies of main window without
  runing several EXEs, this causes:
	* If chashed one main window propably will chrash whole
        program.
	* By incomprehensible reason doesn't work first level of menu 
	accelerator keys. I working on that.
	* Is not posible to switch betwen copies of main window by
        ALT+TAB
	* If you open some dialog window you can't switch to others
	windows.
	* If you change paramaters of connection in one window,
        changes will be immediately visible in others windows of that
        connection.
	* This is decrease system resources consumption.
* On-line help isn't at this moment available.

Version 0.61 (19.03.1998)
=================================
* It's posible to select connection by double click in list.
* If you don't fillin connection comment, host name will be entered as
  comment.

Version 0.60 (03.03.1998)
=================================
* New console. Console was completly rewrited => speed was increased.
* Option "Lazy write" will be no longer available due console change.
  All operations are made in memory and reslut is panited in free
  time.
* Console has scroll memory for 3000 rows. Scrolling is posible by 
  scrollbar or keyboard ALT+Up, Down, Home, End, PageUp, PageDown.
* Consumption of system resources was reduced. Dialog windows are
  allocated on demand. 
* Is posible to write memory of console to a file (ANSI or TXT).
* Czech encoding is fixed. New choice "Keyboad and cliboard charset".

Version 0.53 
=================================
* First release
